| coresightps_dcc Vitis Drivers API Documentation

- Overview
- APIs
- File List

Functions
Overview

## Functions
void | XCoresightPs_DccSendByte (u32 BaseAddress, u8 Data)
| This functions sends a single byte using the DCC. More...
u8 | XCoresightPs_DccRecvByte (u32 BaseAddress)
| This functions receives a single byte using the DCC. More...

## Function Documentation

u8 XCoresightPs_DccRecvByte | ( | u32 | BaseAddress | ) |

This functions receives a single byte using the DCC.

It is blocking in that it waits for the receiver to become non-empty before it reads from the receive register.

Parameters

  BaseAddress | is a dummy parameter to match the function proto of functions for other stdio devices.

Returns
  The byte of data received.

Note
  None.

void XCoresightPs_DccSendByte | ( | u32 | BaseAddress,
|  | u8 | Data
| ) |  |

This functions sends a single byte using the DCC.

It is blocking in that it waits for the transmitter to become non-full before it writes the byte to the transmit register.

Parameters

  BaseAddress | is a dummy parameter to match the function proto of functions for other stdio devices.
  Data | is the byte of data to send

Returns
  None.

Note
  None.