| csi2tx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XCsi2Tx_SPktData Struct Reference
Overview

This typedef contains the Short Packet information from the Generic Short Packet Register. More...

## Data Fields
u16 | Data
| The Data from Camera Sensor. More...
u8 | DataType
| The Data type like RGB, RAW or YUV format. More...
u8 | VirtualChannel
| Virtual Channel on which this short packet is sent. More...

## Detailed Description

This typedef contains the Short Packet information from the Generic Short Packet Register.

## Field Documentation

u16 XCsi2Tx_SPktData::Data

The Data from Camera Sensor.

Referenced by XCsi2Tx_GetShortPacket().

u8 XCsi2Tx_SPktData::DataType

The Data type like RGB, RAW or YUV format.

Referenced by XCsi2Tx_GetShortPacket().

u8 XCsi2Tx_SPktData::VirtualChannel

Virtual Channel on which this short packet is sent.

Referenced by XCsi2Tx_GetShortPacket().