| emaclite Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xemaclite_l.c File Reference

## Functions
void | XEmacLite_AlignedWrite (void *SrcPtr, UINTPTR *DestPtr, unsigned ByteCount)
| This function aligns the incoming data and writes it out to a 32-bit aligned destination address range. More...
void | XEmacLite_AlignedRead (UINTPTR *SrcPtr, void *DestPtr, unsigned ByteCount)
| This function reads from a 32-bit aligned source address range and aligns the writes to the provided destination pointer alignment. More...
void | XEmacLite_SendFrame (UINTPTR BaseAddress, u8 *FramePtr, unsigned ByteCount)
| Send an Ethernet frame. More...
u16 | XEmacLite_RecvFrame (UINTPTR BaseAddress, u8 *FramePtr)
| Receive a frame. More...