| v_gamma_lut Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_gamma_lut Struct Reference

Driver instance data. More...

## Data Fields
XV_gamma_lut_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...
void * | CallbackDoneRef
| To be passed to the connect interrupt callback. More...
void * | CallbackReadyRef
    To be passed to the connect interrupt
callback More...

## Detailed Description

Driver instance data.

An instance must be allocated for each core in use.

## Field Documentation

void* XV_gamma_lut::CallbackDoneRef

To be passed to the connect interrupt callback.

Referenced by XVGammaLut_InterruptHandler(), and XVGammaLut_SetCallback().

void* XV_gamma_lut::CallbackReadyRef

    To be passed to the connect interrupt

callback

Referenced by XVGammaLut_InterruptHandler(), and XVGammaLut_SetCallback().

XV_gamma_lut_Config XV_gamma_lut::Config

Hardware Configuration.

u32 XV_gamma_lut::IsReady

Device is initialized and ready.

Referenced by XVGammaLut_InterruptHandler().