| aiengine Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

xaietile_strm.h File Reference

## Overview

Header file for stream switch configuration.

    MODIFICATION HISTORY:

    Ver   Who     Date     Changes

    1.0  Naresh  04/06/2018  Initial creation
    1.1  Naresh  07/11/2018  Updated copyright info
    1.2  Hyun    10/03/2018  Added the event port select function
    1.3  Hyun    10/08/2018  Added the offset for shim trace slave port
    1.4  Nishad  12/05/2018  Renamed ME attributes to AIE
    1.5  Wendy   16/05/2019  Wrap pointers parameters with () in macro

#define | XAIETILE_STRSW_MPORT_CFGPKT(TileInstPtr, Master, DropHdr, Msk, Arbiter)
| Macro to frame the configuration word for the Master port. More...
#define | XAIETILE_STRSW_SLVSLOT_CFG(TileInstPtr, Slave, SlotIdx, SlotId,SlotMask, SlotEnable, SlotMsel, SlotArbiter)
| Macro to frame the configuration word for the slave port slot register. More...
#define | XAIETILE_STRSW_SPORT_CORE(TileInstPtr, Idx) (XAIETILE_TILESTRSW_SPORT_CORE_OFF + Idx)
| Macro to compute the ID value of stream switch slave port-Core. More...
#define | XAIETILE_STRSW_SPORT_DMA(TileInstPtr, Idx) (XAIETILE_TILESTRSW_SPORT_DMA_OFF + Idx)
| Macro to compute the ID value of stream switch slave port-DMA. More...
#define | XAIETILE_STRSW_SPORT_CTRL(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-Ctrl. More...
#define | XAIETILE_STRSW_SPORT_FIFO(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-FIFO. More...
#define | XAIETILE_STRSW_SPORT_SOUTH(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-South. More...
#define | XAIETILE_STRSW_SPORT_WEST(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-West. More...
#define | XAIETILE_STRSW_SPORT_NORTH(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-North. More...
#define | XAIETILE_STRSW_SPORT_EAST(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-East. More...
#define | XAIETILE_STRSW_SPORT_TRACE(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch slave port-Trace. More...
#define | XAIETILE_STRSW_MPORT_CORE(TileInstPtr, Idx) (XAIETILE_TILESTRSW_MPORT_CORE_OFF + Idx)
| Macro to compute the ID value of stream switch master port-Core. More...
#define | XAIETILE_STRSW_MPORT_DMA(TileInstPtr, Idx) (XAIETILE_TILESTRSW_MPORT_DMA_OFF + Idx)
| Macro to compute the ID value of stream switch master port-DMA. More...
#define | XAIETILE_STRSW_MPORT_CTRL(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-Ctrl. More...
#define | XAIETILE_STRSW_MPORT_FIFO(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-FIFO. More...
#define | XAIETILE_STRSW_MPORT_SOUTH(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-South. More...
#define | XAIETILE_STRSW_MPORT_WEST(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-West. More...
#define | XAIETILE_STRSW_MPORT_NORTH(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-North. More...
#define | XAIETILE_STRSW_MPORT_EAST(TileInstPtr, Idx)
| Macro to compute the ID value of stream switch master port-East. More...
#define | XAIETILE_STRSW_MPORT_TRACE(TileInstPtr, Idx) (XAIETILE_TILESTRSW_MPORT_TRACE_OFF + Idx)
| Macro to compute the ID value of stream switch master port-Trace. More...
void | XAieTile_StrmConnectCct (XAieGbl_Tile *TileInstPtr, u8 Slave, u8 Master, u8 SlvEnable)
| This API is used to connect the selected master port to the specified slave port of the stream switch. More...
void | XAieTile_StrmConfigMstr (XAieGbl_Tile *TileInstPtr, u8 Master, u8 Enable, u8 PktEnable, u8 Config)
| This API is used to configure the selected master port of the stream switch in the corresponding tile as per the parameters. More...
void | XAieTile_StrmConfigSlv (XAieGbl_Tile *TileInstPtr, u8 Slave, u8 Enable, u8 PktEnable)
| This API is used to configure the selected slave port of the stream switch in the corresponding tile. More...
void | XAieTile_StrmConfigSlvSlot (XAieGbl_Tile *TileInstPtr, u8 Slave, u8 Slot, u8 Enable, u32 RegVal)
| This API is used to configure the selected slot of the slave port in the stream switch of the corresponding tile. More...
void | XAieTile_ShimStrmMuxConfig (XAieGbl_Tile *TileInstPtr, u32 Port, u32 Input)
| This API sets up the mux configuraiton for Shim. More...
void | XAieTile_ShimStrmDemuxConfig (XAieGbl_Tile *TileInstPtr, u32 Port, u32 Output)
| This API sets up the mux configuraiton for Shim DMA. More...
void | XAieTile_StrmEventPortSelect (XAieGbl_Tile *TileInstPtr, u8 Port, u8 Master, u8 Id)
| This API sets up the event port in stream switch. More...

## Macro Definition Documentation

#define XAIETILE_STRSW_MPORT_CFGPKT | ( |  | TileInstPtr,
|  |  | Master,
|  |  | DropHdr,
|  |  | Msk,
|  |  | Arbiter
| ) |  |

Value:
({ \
XAieGbl_RegStrmMstr *TmpPtr; \
TmpPtr = ((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
&TileStrmMstr[Master]:&ShimStrmMstr[Master]; \
(XAie_SetField(DropHdr, TmpPtr->DrpHdr.Lsb, TmpPtr->DrpHdr.Mask) | \
((u32)Msk << XAIETILE_STRSW_MPORT_PKTMSEL_SHIFT) | \
((u32)Arbiter << XAIETILE_STRSW_MPORT_PKTARB_SHIFT)); \
})

Macro to frame the configuration word for the Master port.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Master | - Master port ID value.
  DropHdr | - Drop header on packet.
  Msk | - Mask to be used on packet ID.
  Arbiter | - Arbiter to use when packet matches.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_MPORT_CORE | ( |  | TileInstPtr,
|  |  | Idx
| ) |  | (XAIETILE_TILESTRSW_MPORT_CORE_OFF + Idx)

Macro to compute the ID value of stream switch master port-Core.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_MPORT_CTRL | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_CTRL_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_CTRL_OFF + Idx)

Macro to compute the ID value of stream switch master port-Ctrl.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_MPORT_DMA | ( |  | TileInstPtr,
|  |  | Idx
| ) |  | (XAIETILE_TILESTRSW_MPORT_DMA_OFF + Idx)

Macro to compute the ID value of stream switch master port-DMA.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_MPORT_EAST | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_EAST_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_EAST_OFF + Idx)

Macro to compute the ID value of stream switch master port-East.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_MPORT_FIFO | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_FIFO_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_FIFO_OFF + Idx)

Macro to compute the ID value of stream switch master port-FIFO.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_MPORT_NORTH | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_NORTH_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_NORTH_OFF + Idx)

Macro to compute the ID value of stream switch master port-North.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_MPORT_SOUTH | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_SOUTH_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_SOUTH_OFF + Idx)

Macro to compute the ID value of stream switch master port-South.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_MPORT_TRACE | ( |  | TileInstPtr,
|  |  | Idx
| ) |  | (XAIETILE_TILESTRSW_MPORT_TRACE_OFF + Idx)

Macro to compute the ID value of stream switch master port-Trace.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_MPORT_WEST | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_MPORT_WEST_OFF + Idx): \
(XAIETILE_SHIMSTRSW_MPORT_WEST_OFF + Idx)

Macro to compute the ID value of stream switch master port-West.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SLVSLOT_CFG | ( |  | TileInstPtr,
|  |  | Slave,
|  |  | SlotIdx,
|  |  | SlotId,
|  |  | SlotMask,
|  |  | SlotEnable,
|  |  | SlotMsel,
|  |  | SlotArbiter
| ) |  |

Value:
({ \
XAieGbl_RegStrmSlot *TmpPtr; \
TmpPtr = (((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
&TileStrmSlot[XAIETILE_STRSW_SPORT_NUMSLOTS*Slave + SlotIdx]: \
&ShimStrmSlot[XAIETILE_STRSW_SPORT_NUMSLOTS*Slave + SlotIdx]); \
(XAie_SetField(SlotId, TmpPtr->Id.Lsb, TmpPtr->Id.Mask) | \
XAie_SetField(SlotMask, TmpPtr->Mask.Lsb, TmpPtr->Mask.Mask) | \
XAie_SetField(SlotEnable, TmpPtr->En.Lsb, TmpPtr->En.Mask) | \
XAie_SetField(SlotMsel, TmpPtr->Msel.Lsb, TmpPtr->Msel.Mask) | \
XAie_SetField(SlotArbiter, TmpPtr->Arb.Lsb, TmpPtr->Arb.Mask)); \
})

Macro to frame the configuration word for the slave port slot register.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Slave | - Slave port ID value.
  SlotIdx | - Slave slot ID value, ranging from 0-3.
  SlotId | - Slot ID value.
  SlotMask | - Slot mask value.
  SlotEnable | - Slot enable (1-Enable,0-Disable).
  SlotMsel | - master select.
  SlotArbiter | - Arbiter to use.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_SPORT_CORE | ( |  | TileInstPtr,
|  |  | Idx
| ) |  | (XAIETILE_TILESTRSW_SPORT_CORE_OFF + Idx)

Macro to compute the ID value of stream switch slave port-Core.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SPORT_CTRL | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_CTRL_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_CTRL_OFF + Idx)

Macro to compute the ID value of stream switch slave port-Ctrl.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SPORT_DMA | ( |  | TileInstPtr,
|  |  | Idx
| ) |  | (XAIETILE_TILESTRSW_SPORT_DMA_OFF + Idx)

Macro to compute the ID value of stream switch slave port-DMA.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_SPORT_EAST | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_EAST_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_EAST_OFF + Idx)

Macro to compute the ID value of stream switch slave port-East.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SPORT_FIFO | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_FIFO_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_FIFO_OFF + Idx)

Macro to compute the ID value of stream switch slave port-FIFO.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SPORT_NORTH | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_NORTH_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_NORTH_OFF + Idx)

Macro to compute the ID value of stream switch slave port-North.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_SPORT_SOUTH | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_SOUTH_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_SOUTH_OFF + Idx)

Macro to compute the ID value of stream switch slave port-South.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

Referenced by main().

#define XAIETILE_STRSW_SPORT_TRACE | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_TRACE_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_TRACE_OFF + Idx)

Macro to compute the ID value of stream switch slave port-Trace.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

#define XAIETILE_STRSW_SPORT_WEST | ( |  | TileInstPtr,
|  |  | Idx
| ) |  |

Value:
((TileInstPtr)->TileType == XAIEGBL_TILE_TYPE_AIETILE)? \
(XAIETILE_TILESTRSW_SPORT_WEST_OFF + Idx): \
(XAIETILE_SHIMSTRSW_SPORT_WEST_OFF + Idx)

Macro to compute the ID value of stream switch slave port-West.

Parameters

  TileInstPtr | - Tile instance pointer.
  Idx | - Index value.

Returns
  None.

Note
  None.

## Function Documentation

void XAieTile_ShimStrmDemuxConfig | ( | XAieGbl_Tile * | TileInstPtr,
|  | u32 | Port,
|  | u32 | Output
| ) |  |

This API sets up the mux configuraiton for Shim DMA.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Port,: | Should be one of XAIETILE_SHIM_STRM_DEM_SOUTH2, XAIETILE_SHIM_STRM_DEM_SOUTH3, XAIETILE_SHIM_STRM_DEM_SOUTH4, or XAIETILE_SHIM_STRM_DEM_SOUTH5
  Output,: | Should be one of XAIETILE_SHIM_STRM_DEM_PL, XAIETILE_SHIM_STRM_DEM_DMA, or XAIETILE_SHIM_STRM_DEM_NOC.

Returns
  None.

Note
  None.

References XAieGbl_RegShimDemCfg::CtrlOff, XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegShimDemCfg::Port, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.

void XAieTile_ShimStrmMuxConfig | ( | XAieGbl_Tile * | TileInstPtr,
|  | u32 | Port,
|  | u32 | Input
| ) |  |

This API sets up the mux configuraiton for Shim.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Port,: | Should be one of XAIETILE_SHIM_STRM_MUX_SOUTH2, XAIETILE_SHIM_STRM_MUX_SOUTH3, XAIETILE_SHIM_STRM_MUX_SOUTH6, or XAIETILE_SHIM_STRM_MUX_SOUTH7
  Input,: | Should be one of XAIETILE_SHIM_STRM_MUX_PL, XAIETILE_SHIM_STRM_MUX_DMA, or XAIETILE_SHIM_STRM_MUX_NOC.

Returns
  None.

Note
  None.

References XAieGbl_RegShimMuxCfg::CtrlOff, XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegShimMuxCfg::Port, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.

void XAieTile_StrmConfigMstr | ( | XAieGbl_Tile * | TileInstPtr,
|  | u8 | Master,
|  | u8 | Enable,
|  | u8 | PktEnable,
|  | u8 | Config
| ) |  |

This API is used to configure the selected master port of the stream switch in the corresponding tile as per the parameters.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Master | - Master port ID value.
  Enable | - Enable/Disable the master port (1-Enable,0-Disable).
  PktEnable | - Enable/Disable the packet switching mode (1-Enable,0-Disable).
  Config | - Config value to be used for circuit/packet sw. Applicable only when Enable==1. Bit encoding when PktEnable==1: 7-Drop header on packet, 6:3-Mask, 2:0-Arbiter Bit encoding when PktEnable==0: 7:5-Rsvd, 4:0-Slave port ID to which the master port need to connect to Use the macro "xaietile_strm.c::XAIETILE_STRSW_MPORT_CFGPKT()" to frame the 8-bit Config.

Returns
  None.

Note
  None.

References XAieGbl_RegStrmMstr::Config, XAieGbl_RegStrmMstr::DrpHdr, XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegStrmMstr::MstrEn, XAieGbl_RegStrmMstr::PktEn, XAieGbl_RegStrmMstr::RegOff, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.

Referenced by main(), and XAieTile_StrmConnectCct().

void XAieTile_StrmConfigSlv | ( | XAieGbl_Tile * | TileInstPtr,
|  | u8 | Slave,
|  | u8 | Enable,
|  | u8 | PktEnable
| ) |  |

This API is used to configure the selected slave port of the stream switch in the corresponding tile.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Slave | - Slave port ID value.
  Enable | - Enable/Disable the slave port (1-Enable,0-Disable).
  PktEnable | - Enable/Disable the packet switching mode (1-Enable,0-Disable).

Returns
  None.

Note
  None.

References XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegStrmSlv::PktEn, XAieGbl_RegStrmSlv::RegOff, XAieGbl_RegStrmSlv::SlvEn, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.

Referenced by main(), and XAieTile_StrmConnectCct().

void XAieTile_StrmConfigSlvSlot | ( | XAieGbl_Tile * | TileInstPtr,
|  | u8 | Slave,
|  | u8 | Slot,
|  | u8 | Enable,
|  | u32 | RegVal
| ) |  |

This API is used to configure the selected slot of the slave port in the stream switch of the corresponding tile.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Slave | - Slave port ID value.
  Slot | - Slave slot ID value, ranging from 0-3.
  Enable | - Enable/Disable the slave slot (1-Enable,0-Disable).
  RegVal | - Config value to be used for the slot. Applicable only when Enable==1, else set to 0. Bit encoding : 31:21-Rsvd, 28:24-Slot ID, 23:21-Rsvd, 20:16-ID mask, 15:6-Rsvd, 5:4-Master select/msel, 3-Rsvd, 2:0-Arbiter to use. Use the macro "xaietile_strm.c::XAIETILE_STRSW_SLVSLOT_CFG()" to frame the 32-bit RegVal.

Returns
  None.

Note
  None.

References XAieGbl_RegStrmSlot::En, XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegStrmSlot::RegOff, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.

Referenced by main().

void XAieTile_StrmConnectCct | ( | XAieGbl_Tile * | TileInstPtr,
|  | u8 | Slave,
|  | u8 | Master,
|  | u8 | SlvEnable
| ) |  |

This API is used to connect the selected master port to the specified slave port of the stream switch.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Slave | - slave port ID value.
  Master | - Master port ID value.
  SlvEnable | - Enable/Disable the slave port (1-Enable,0-Disable).

Returns
  None.

Note
  None.

References XAieTile_StrmConfigMstr(), and XAieTile_StrmConfigSlv().

Referenced by main().

void XAieTile_StrmEventPortSelect | ( | XAieGbl_Tile * | TileInstPtr,
|  | u8 | Port,
|  | u8 | Master,
|  | u8 | Id
| ) |  |

This API sets up the event port in stream switch.

Parameters

  TileInstPtr | - Pointer to the Tile instance.
  Port,: | Port number. 0 to 7.
  Master,: | 1 for master. 0 for slave.
  Id,: | Port ID for event generation

Returns
  None.

Note
  None.

References XAieGbl_RegFldAttr::Lsb, XAieGbl_RegFldAttr::Mask, XAieGbl_RegStrmEvtPort::MstrSlv, XAieGbl_RegStrmEvtPort::Port, XAieGbl_RegStrmEvtPort::RegOff, XAieGbl_Tile::TileAddr, and XAieGbl_Tile::TileType.