| mipicsiss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
si5344drv.c File Reference

## Overview

This file contains the Xilinx Menu implementation as used in the HDMI example design.

Please see xhdmi_menu.h for more details.

    MODIFICATION HISTORY:

    Ver   Who  Date       Changes

    X.X   ..   DD-MM-YYYY ..
    1.0        23-07-2019 Initial version

## Functions
int | SI5344_Init (void *IicPtr, u8 I2CSlaveAddress)
| This function initializes the SI 5344 device. More...

## Function Documentation

int SI5344_Init | ( | void * | IicPtr,
|  | u8 | I2CSlaveAddress
| ) |  |

This function initializes the SI 5344 device.

Parameters

  I2CBaseAddress | is the baseaddress of the I2C core.
  I2CSlaveAddress | is the 7-bit I2C slave address.

Returns
  - XST_SUCCESS Initialization was successful.
  - XST_FAILURE I2C write error.

Note
  None.