| mipicsiss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Macros | Typedefs | Functions
xcsiss.h File Reference

## Data Structures
struct | CsiRxSsSubCore
| Sub-Core Configuration Table. More...
struct | XCsiSs_Config
| MIPI CSI Rx Subsystem configuration structure. More...
struct | XCsiSs
| The XCsiSs driver instance data. More...

## Macros
#define | XCSISS_H_
| Prevent circular inclusions by using protection macros. More...
Interrupt Types for setting Callbacks
These handlers are used to determine the type of the interrupt handler being registered with the MIPI CSI Rx Subsystem. Since the subsystem is tightly coupled with the CSI Rx Controller driver, the handlers from the sub core are promoted to the subsystem level so that the application can use them.
#define | XCSISS_HANDLER_DPHY XCSI_HANDLER_DPHY
#define | XCSISS_HANDLER_PKTLVL XCSI_HANDLER_PKTLVL
#define | XCSISS_HANDLER_PROTLVL XCSI_HANDLER_PROTLVL
#define | XCSISS_HANDLER_SHORTPACKET XCSI_HANDLER_SHORTPACKET
#define | XCSISS_HANDLER_FRAMERECVD XCSI_HANDLER_FRAMERECVD
#define | XCSISS_HANDLER_OTHERERROR XCSI_HANDLER_OTHERERROR
#define | XCSISS_HANDLER_VCX XCSI_HANDLER_VCXFRAMEERROR

## Typedefs
typedef void(* | XCsiSs_Callback )(void *CallbackRef, u32 Mask)
| Callback type which acts as a wrapper on top of CSI Callback. More...

## Functions
XCsiSs_Config * | XCsiSs_LookupConfig (u32 DeviceId)
| This function looks for the device configuration based on the unique device ID. More...
u32 | XCsiSs_CfgInitialize (XCsiSs *InstancePtr, XCsiSs_Config *CfgPtr, UINTPTR EffectiveAddr)
| This function initializes the MIPI CSI subsystem and included sub-cores. More...
u32 | XCsiSs_Configure (XCsiSs *InstancePtr, u8 ActiveLanes, u32 IntrMask)
| This function is used to configure the CSI lanes and interrupts that are to be handled by the application. More...
u32 | XCsiSs_Activate (XCsiSs *InstancePtr, u8 Flag)
| This function is used to activate the CSI Subsystem. More...
u32 | XCsiSs_Reset (XCsiSs *InstancePtr)
| This function is used to reset the CSI Subsystem. More...
void | XCsiSs_ReportCoreInfo (XCsiSs *InstancePtr)
| This function reports list of cores included. More...
void | XCsiSs_GetLaneInfo (XCsiSs *InstancePtr)
| This function gets the clk and data lane info. More...
void | XCsiSs_GetShortPacket (XCsiSs *InstancePtr)
| This function gets the short packets. More...
void | XCsiSs_GetVCInfo (XCsiSs *InstancePtr)
| This function gets the virtual channel information. More...
u32 | XCsiSs_GetVCSelection (XCsiSs *InstancePtr)
| This function will return the virtual channels selected. More...
void | XCsiSs_SetVCSelection (XCsiSs *InstancePtr, u16 Value)
| This function will control the virtual channels selection dynamically. More...
u32 | XCsiSs_SelfTest (XCsiSs *InstancePtr)
| This function performs self test on MIPI CSI Rx Subsystem sub-cores. More...
void | XCsiSs_IntrHandler (void *InstancePtr)
| This function is the interrupt handler for the MIPI CSI Rx Subsystem. More...
void | XCsiSs_IntrDisable (XCsiSs *InstancePtr, u32 IntrMask)
| This function is used to disable the interrupts in the CSI core. More...
u32 | XCsiSs_SetCallBack (XCsiSs *InstancePtr, u32 HandlerType, void *CallbackFunc, void *CallbackRef)
| This routine installs an asynchronous callback function for the given HandlerType: More...