| hdcp22_tx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XHdcp22_Tx_Timer Struct Reference
Overview

The current state and data for internal used timer. More...

## Data Fields
u8 | TimerExpired
| Expiration flag set when the hardware timer has interrupted. More...
u8 | ReasonId
| Keep track of why the timer was started (message or status checking). More...
u32 | InitialTicks
| Keep track of the start value of the timer. More...
XTmrCtr | TmrCtr
| The hardware timer instance. More...

## Detailed Description

The current state and data for internal used timer.

## Field Documentation

u32 XHdcp22_Tx_Timer::InitialTicks

Keep track of the start value of the timer.

Referenced by XHdcp22Tx_CfgInitialize().

u8 XHdcp22_Tx_Timer::ReasonId

Keep track of why the timer was started (message or status checking).

Referenced by XHdcp22Tx_CfgInitialize().

u8 XHdcp22_Tx_Timer::TimerExpired

Expiration flag set when the hardware timer has interrupted.

Referenced by XHdcp22Tx_CfgInitialize(), and XHdcp22Tx_Poll().

XTmrCtr XHdcp22_Tx_Timer::TmrCtr

The hardware timer instance.

Referenced by XHdcp22Tx_Enable(), XHdcp22Tx_GetTimer(), XHdcp22Tx_LogGetTimeUSecs(), XHdcp22Tx_LogReset(), and XHdcp22Tx_Reset().