| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_InternalChannelCfg Struct Reference
Overview

Full RC configuration. More...

## Data Fields
u32 | Enable
| [0,1] Indicates if this RCID is enabled. More...
u32 | RCId
       [0-15] RCCID number allocated to this RACH channel
configuration. More...
u32 | RachChannel
              [0-15] The physical RACH channel used by this
RCID. More...
s32 | CCID
       [0-15] The CCID channel (within the band defined in
field BAND) from which this RACH channel is to be extracted. More...
u32 | BandId
         [0-2] The Band from which this RACH channel is to be
extracted. More...

## Detailed Description

Full RC configuration.

## Field Documentation

u32 XDfePrach_InternalChannelCfg::BandId

         [0-2] The Band from which this RACH channel is to be

extracted.

s32 XDfePrach_InternalChannelCfg::CCID

       [0-15] The CCID channel (within the band defined in

field BAND) from which this RACH channel is to be extracted.

u32 XDfePrach_InternalChannelCfg::Enable

[0,1] Indicates if this RCID is enabled.

u32 XDfePrach_InternalChannelCfg::RachChannel

              [0-15] The physical RACH channel used by this

RCID.

u32 XDfePrach_InternalChannelCfg::RCId

       [0-15] RCCID number allocated to this RACH channel

configuration.

This is the TID identifier on the RACH/FFT interface.