| hwicap Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Examples

You can refer to the below stated example applications for more details on how to use hwicap driver.

# xhwicap_intr_example.c

Contains an example on how to use the XHwicap driver directly. This example shows the usage of the driver in interrupt mode.

For details, see xhwicap_intr_example.c.

# xhwicap_low_level_example.c

Contains an example on how to use the XHwicap driver directly. This example shows the usage of the low-level macros and functions of the hwicap driver.

For details, see xhwicap_low_level_example.c.

# xhwicap_read_config_reg.c

Contains an example on how to use the XHwicap driver directly. This example prints out the values of all the configuration registers in the FPGA.

For details, see xhwicap_read_config_reg.c.

# xhwicap_read_frame_polled_example.c

Contains an example on how to use the XHwicap driver directly. This example shows the usage of the driver to read one frame from the device using the polled mode.

For details, see xhwicap_read_frame_polled_example.c.

# xhwicap_testapp_example.c

Contains an example on how to use the XHwicap driver directly. This example shows the usage of the hwicap driver.

For details, see xhwicap_testapp_example.c.