| dsirxss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDsi2RxSs_Config Struct Reference
Overview

MIPI DSI Rx Subsystem configuration structure. More...

## Data Fields
UINTPTR | BaseAddr
        BaseAddress is the physical
base address of the subsystem address range More...
UINTPTR | HighAddr
        HighAddress is the physical
MAX address of the subsystem address range More...
u8 | DataType
| RGB type. More...
u8 | DsiPixel
| Pixels per beat received on input stream. More...
u32 | DphyLinerate
| DPHY line rate. More...
u32 | IsDphyRegIntfcPresent
    Flag for DPHY register
interface presence More...
Dsi2RxSsSubCores | DphyInfo
| Sub-core instance configuration. More...
Dsi2RxSsSubCores | Dsi2RxInfo
| Sub-core instance configuration. More...

## Detailed Description

MIPI DSI Rx Subsystem configuration structure.

Each subsystem device should have a configuration structure associated that defines the MAX supported sub-cores within subsystem

## Field Documentation

UINTPTR XDsi2RxSs_Config::BaseAddr

        BaseAddress is the physical

base address of the subsystem address range

Referenced by Dsi2RxSs_SelfTestExample(), and XDsi2RxSs_CfgInitialize().

u8 XDsi2RxSs_Config::DataType

RGB type.

Dsi2RxSsSubCores XDsi2RxSs_Config::DphyInfo

Sub-core instance configuration.

Referenced by XDsi2RxSs_ReportCoreInfo().

u32 XDsi2RxSs_Config::DphyLinerate

DPHY line rate.

Dsi2RxSsSubCores XDsi2RxSs_Config::Dsi2RxInfo

Sub-core instance configuration.

u8 XDsi2RxSs_Config::DsiPixel

Pixels per beat received on input stream.

UINTPTR XDsi2RxSs_Config::HighAddr

        HighAddress is the physical

MAX address of the subsystem address range

u32 XDsi2RxSs_Config::IsDphyRegIntfcPresent

    Flag for DPHY register

interface presence

Referenced by XDsi2RxSs_Reset().