| v_hdmitx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_HdmiTx_Config Struct Reference

This typedef contains configuration information for the HDMI TX core. More...

## Data Fields
u16 | DeviceId
| DeviceId is the unique ID of the HDMI TX core. More...
UINTPTR | BaseAddress
       BaseAddress is the physical
base address of the core's registers More...

## Detailed Description

This typedef contains configuration information for the HDMI TX core.

Each HDMI TX device should have a configuration structure associated.

## Field Documentation

UINTPTR XV_HdmiTx_Config::BaseAddress

       BaseAddress is the physical

base address of the core's registers

Referenced by XV_HdmiTx_AuxSend(), XV_HdmiTx_CfgInitialize(), XV_HdmiTx_DdcGetAck(), XV_HdmiTx_DdcInit(), XV_HdmiTx_DdcReadData(), XV_HdmiTx_DdcWaitForDone(), XV_HdmiTx_DdcWriteCommand(), XV_HdmiTx_IntrHandler(), XV_HdmiTx_SelfTest(), XV_HdmiTx_SetColorDepth(), XV_HdmiTx_SetColorFormat(), XV_HdmiTx_SetPixelRate(), and XV_HdmiTx_SetSampleRate().

u16 XV_HdmiTx_Config::DeviceId

DeviceId is the unique ID of the HDMI TX core.