| uartpsv Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XUartPsvFormat Struct Reference
Overview

Keep track of data format setting of a device. More...

## Data Fields
u32 | BaudRate
| In bps, ie 1200. More...
u32 | DataBits
| Number of data bits. More...
u32 | Parity
| Parity. More...
u8 | StopBits
| Number of stop bits. More...

## Detailed Description

Keep track of data format setting of a device.

## Field Documentation

u32 XUartPsvFormat::BaudRate

In bps, ie 1200.

Referenced by XUartPsv_GetDataFormat(), and XUartPsv_SetDataFormat().

u32 XUartPsvFormat::DataBits

Number of data bits.

Referenced by XUartPsv_GetDataFormat(), and XUartPsv_SetDataFormat().

u32 XUartPsvFormat::Parity

Parity.

Referenced by XUartPsv_GetDataFormat(), and XUartPsv_SetDataFormat().

u8 XUartPsvFormat::StopBits

Number of stop bits.

Referenced by XUartPsv_GetDataFormat(), and XUartPsv_SetDataFormat().