| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_MixerStatusOverrun Struct Reference
Overview

PRACH mixer overflow status. More...

## Data Fields
u32 | MixerOverrun
               [0-1] Source of first occurrence of selector
overrun as signalled in ISR. More...
u32 | FirstAntennaOverruning
                         [0-7] Earliest antenna in which
selector overrun occurred. More...
u32 | FirstRCIdOverruning
                      [0-15] Lowest numbered Physical RACH
channel on which first selector overrun occurred. More...

## Detailed Description

PRACH mixer overflow status.

## Field Documentation

u32 XDfePrach_MixerStatusOverrun::FirstAntennaOverruning

                         [0-7] Earliest antenna in which

selector overrun occurred.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_MixerStatusOverrun::FirstRCIdOverruning

                      [0-15] Lowest numbered Physical RACH

channel on which first selector overrun occurred.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_MixerStatusOverrun::MixerOverrun

               [0-1] Source of first occurrence of selector

overrun as signalled in ISR.

That is, register only updated when SELECTOR_OVERRUN flag is 0.

Referenced by XDfePrach_GetStatus().