| v_demosaic Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_demosaic Struct Reference

Driver instance data. More...

## Data Fields
XV_demosaic_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...
void * | CallbackDoneRef
| To be passed to the connect interrupt callback. More...
void * | CallbackReadyRef
    To be passed to the connect interrupt
callback More...

## Detailed Description

Driver instance data.

An instance must be allocated for each core in use.

## Field Documentation

void* XV_demosaic::CallbackDoneRef

To be passed to the connect interrupt callback.

Referenced by XVDemosaic_InterruptHandler(), and XVDemosaic_SetCallback().

void* XV_demosaic::CallbackReadyRef

    To be passed to the connect interrupt

callback

Referenced by XVDemosaic_InterruptHandler(), and XVDemosaic_SetCallback().

XV_demosaic_Config XV_demosaic::Config

Hardware Configuration.

u32 XV_demosaic::IsReady

Device is initialized and ready.

Referenced by XVDemosaic_InterruptHandler().