| iomodule Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xiomodule_l.c File Reference

## Functions
void | XIOModule_DeviceInterruptHandler (void *DeviceId)
| This function is the primary interrupt handler for the driver. More...
void | XIOModule_SetIntrSvcOption (UINTPTR BaseAddress, s32 Option)
| Set the interrupt service option, which can configure the driver so that it services only a single interrupt at a time when an interrupt occurs, or services all pending interrupts when an interrupt occurs. More...
void | XIOModule_RegisterHandler (UINTPTR BaseAddress, s32 InterruptId, XInterruptHandler Handler, void *CallBackRef)
| Register a handler function for a specific interrupt ID. More...
void | XIOModule_SendByte (UINTPTR BaseAddress, u8 Data)
| This functions sends a single byte using the UART. More...
u8 | XIOModule_RecvByte (UINTPTR BaseAddress)
| This functions receives a single byte using the UART. More...