| rfdc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

xrfdc_clk.c File Reference

## Overview

This file contains a programming example for using the lmx2594 and lmk04028 clock generator.

This example configures the lmx2594 to 20 frequencies. If 0 is passed then the chip is powered down. For zcu111 board users are expected to define XPS_BOARD_ZCU111 macro while compiling this example.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes

    1.0   sd     04/11/18 First release
    4.0   sd     05/22/18 Updated lmx configuration
    5.0   sd     09/05/18 Updated lmx reset sequence
    8.0   cog    04/09/20 Fixed error in PLL B for 1474.56 MHz