| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Examples

You can refer to the below stated example applications for more details on how to use the driver.

# xdfemix_examples.c

Examples are:

1. Self test on one instance:
   - initialisation from reset to activation
   - close the driver
2. Initialise and set one instance of XDfeMix driver in pass through mode.
   - initialisation from reset to activation
   - configure mixer in pass true mode
   - close the driver

The example code is written and tested for zcu670 board. Running example in a Bare metal environment includes setting an output clock on si570. For details, see xdfemix examples code.