| gpio Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XGpio_Config Struct Reference
GPIO APIs

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| Device base address. More...
int | InterruptPresent
| Are interrupts supported in h/w. More...
int | IsDual
| Are 2 channels supported in h/w. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

UINTPTR XGpio_Config::BaseAddress

Device base address.

Referenced by XGpio_Initialize().

u16 XGpio_Config::DeviceId

Unique ID of device.

int XGpio_Config::InterruptPresent

Are interrupts supported in h/w.

Referenced by XGpio_CfgInitialize().

int XGpio_Config::IsDual

Are 2 channels supported in h/w.

Referenced by XGpio_CfgInitialize().