| sdps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- All
- Functions
- Variables
- Macros

- a
- c
- e
- h
- m
- s
- u
- w
- x

Here is a list of all documented functions, variables, defines, enums, and typedefs with links to the documentation:

### - a -

- ADDRESS_BEYOND_32BIT : xsdps.h

### - c -

- CSD_SPEC_VER_3 : xsdps.h

### - e -

- ENABLE_HS400_MODE : xsdps.h
- EXT_CSD_DEVICE_TYPE_BYTE : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V2_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V2_HS400 : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V8_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_DDR_1V8_HS400 : xsdps.h
- EXT_CSD_DEVICE_TYPE_HIGH_SPEED : xsdps.h
- EXT_CSD_DEVICE_TYPE_SDR_1V2_HS200 : xsdps.h
- EXT_CSD_DEVICE_TYPE_SDR_1V8_HS200 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE1 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE2 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE3 : xsdps.h
- EXT_CSD_SEC_COUNT_BYTE4 : xsdps.h

### - h -

- HIGH_SPEED_SUPPORT : xsdps.h

### - m -

- main() : xsdps_raw_example.c
- MAX_TIMEOUT : xsdps.h
- MAX_TUNING_COUNT : xsdps.h

### - s -

- SCR_SPEC_VER_3 : xsdps.h
- SD_CLK_19_MHZ : xsdps.h
- SD_CLK_25_MHZ : xsdps.h
- SD_CLK_26_MHZ : xsdps.h
- SD_HS_MODE_ENABLE : xsdps.h

### - u -

- UHS_DDR50_SUPPORT : xsdps.h
- UHS_SDR104_SUPPORT : xsdps.h
- UHS_SDR12_SUPPORT : xsdps.h
- UHS_SDR25_SUPPORT : xsdps.h
- UHS_SDR50_SUPPORT : xsdps.h

### - w -

- WIDTH_4_BIT_SUPPORT : xsdps.h

### - x -

- XSDPS_ACMD41_3V3 : xsdps.h
- XSDPS_ACMD41_HCS : xsdps.h
- XSdPs_AutoTuning() : xsdps_card.c
- XSDPS_BLK_SIZE_512_MASK : xsdps.h
- XSdPs_CalcBusSpeed() : xsdps_host.c
- XSdPs_CalcClock() : xsdps_host.c
- XSdPs_CardIfCond() : xsdps_card.c
- XSdPs_CardInitialize() : xsdps.c
- XSdPs_CardOpCond() : xsdps_card.c
- XSdPs_CardReset() : xsdps_card.c
- XSdPs_CardSetVoltage18() : xsdps_card.c
- XSdPs_CfgInitialize() : xsdps.c
- XSdPs_Change_BusSpeed() : xsdps.h
- XSdPs_Change_BusWidth() : xsdps.h
- XSdPs_Change_ClkFreq() : xsdps.h
- XSdPs_Change_MmcBusSpeed() : xsdps_card.c
- XSdPs_Change_SdBusSpeed() : xsdps_card.c
- XSdPs_CheckBusHigh() : xsdps_card.c
- XSdPs_CheckBusIdle() : xsdps_host.c
- XSdPs_CheckCardDetect() : xsdps_card.c
- XSdPs_CheckEmmcTiming() : xsdps_card.c
- XSdPs_CheckReadTransfer() : xsdps.h
- XSdPs_CheckResetDone() : xsdps_card.c
- XSdPs_CheckTransferComplete() : xsdps_card.c
- XSdps_CheckTransferDone() : xsdps_host.c
- XSdPs_CheckVoltage18() : xsdps_card.c
- XSdPs_CheckWriteTransfer() : xsdps.h
- XSDPS_CMD1_DUAL_VOL : xsdps.h
- XSDPS_CMD1_HIGH_VOL : xsdps.h
- XSDPS_CMD8_VOL_PATTERN : xsdps.h
- XSdPs_CmdTransfer() : xsdps_host.c
- XSdPs_ConfigDma() : xsdps_host.c
- XSdPs_ConfigInterrupt() : xsdps_host.c
- XSdPs_ConfigPower() : xsdps_host.c
- XSdPs_ConfigTable : xsdps.h , xsdps_g.c
- XSdPs_ConfigTapDelay() : xsdps_host.c
- XSDPS_CT_ERROR : xsdps.h
- XSdPs_DisableBusPower() : xsdps_host.c
- XSdPs_DllReset() : xsdps_card.c
- XSdPs_DllRstCtrl() : xsdps_host.c
- XSdPs_EmmcModeInit() : xsdps_host.c
- XSdPs_EnableBusPower() : xsdps_host.c
- XSdPs_EnableClock() : xsdps_host.c
- XSdPs_Erase() : xsdps.c
- XSdPs_Execute_Tuning() : xsdps_host.c
- XSdPs_FrameCmd() : xsdps_host.c
- XSdPs_Get_BusSpeed() : xsdps.h
- XSdPs_Get_BusWidth() : xsdps.h
- XSdPs_Get_Mmc_ExtCsd() : xsdps.h
- XSdPs_Get_Status() : xsdps.h
- XSdPs_GetCardId() : xsdps_card.c
- XSdPs_GetCsd() : xsdps_card.c
- XSdPs_HostConfig() : xsdps_card.c
- XSdPs_Identify_UhsMode() : xsdps_card.c
- XSdPs_IdentifyCard() : xsdps_card.c
- XSdPs_IdentifyEmmcMode() : xsdps_card.c
- XSdPs_Idle() : xsdps.c
- XSdPs_LookupConfig() : xsdps.h
- XSdPs_MmcCardEnum() : xsdps_host.c
- XSdPs_MmcCardInitialize() : xsdps_card.c
- XSdPs_MmcModeInit() : xsdps_host.c
- XSdPs_Pullup() : xsdps.h
- XSdPs_Read() : xsdps_card.c
- XSdPs_ReadPolled() : xsdps.c
- XSdPs_Reset() : xsdps_host.c
- XSdPs_ResetConfig() : xsdps_card.c
- XSDPS_RESPOCR_READY : xsdps.h
- XSdPs_Sanitize() : xsdps.c
- XSdPs_SdCardEnum() : xsdps_host.c
- XSdPs_SdCardInitialize() : xsdps_card.c
- XSdPs_SdModeInit() : xsdps_host.c
- XSdPs_Select_Card() : xsdps.h
- XSdPs_SendCmd() : xsdps_card.c
- XSdPs_SendErase() : xsdps_card.c
- XSdPs_Set_Mmc_ExtCsd() : xsdps.h
- XSdPs_SetBlkSize() : xsdps.h
- XSdPs_SetClock() : xsdps_card.c
- XSdPs_SetEndAddr() : xsdps_card.c
- XSdPs_SetExecTuning() : xsdps_host.c
- XSdPs_SetStartAddr() : xsdps_card.c
- XSdPs_SetTapDelay() : xsdps_card.c
- XSdPs_SetTapDelay_DDR50() : xsdps_host.c
- XSdPs_SetTapDelay_SDR104() : xsdps_host.c
- XSdPs_SetTapDelay_SDR25() : xsdps_host.c
- XSdPs_SetTapDelay_SDR50() : xsdps_host.c
- XSdPs_Setup32ADMA2DescTbl() : xsdps_host.c
- XSdPs_Setup64ADMA2DescTbl() : xsdps_host.c
- XSdPs_SetupADMA2DescTbl() : xsdps_card.c
- XSdPs_SetupADMA2DescTbl64Bit() : xsdps_card.c
- XSdPs_SetupCmd() : xsdps_card.c
- XSdPs_SetupReadDma() : xsdps_host.c
- XSdPs_SetupTransfer() : xsdps_host.c
- XSdPs_SetupVoltageSwitch() : xsdps_card.c
- XSdPs_SetupWriteDma() : xsdps_host.c
- XSdPs_SetVoltage18() : xsdps_host.c
- XSdPs_StartReadTransfer() : xsdps.h
- XSdPs_StartWriteTransfer() : xsdps.h
- XSdPs_Switch_Voltage() : xsdps_host.c
- XSDPS_VERSAL_SD0_BASE : xsdps.h
- XSDPS_VERSAL_SD1_BASE : xsdps.h
- XSdPs_Write() : xsdps_card.c
- XSdPs_WritePolled() : xsdps.c
- XSDPS_ZYNQMP_SD0_BASE : xsdps.h
- XSDPS_ZYNQMP_SD1_BASE : xsdps.h