| aiengine Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XAieGbl_RegShimDmaSts Struct Reference

This typedef contains the attributes for Shim DMA status registers. More...

## Data Fields
u32 | RegOff
| Register offset. More...
XAieGbl_RegFldAttr | StartQueueOverflow
| Start queue overflow. More...
XAieGbl_RegFldAttr | CurrentBd
| Current Bd. More...
XAieGbl_RegFldAttr | StartQSize
| Start queue size. More...
XAieGbl_RegFldAttr | Stalled
| If stalled due to lock. More...
XAieGbl_RegFldAttr | Sts
| Status. More...

## Detailed Description

This typedef contains the attributes for Shim DMA status registers.

## Field Documentation

XAieGbl_RegFldAttr XAieGbl_RegShimDmaSts::CurrentBd

Current Bd.

u32 XAieGbl_RegShimDmaSts::RegOff

Register offset.

Referenced by XAieDma_ShimPendingBdCount(), and XAieDma_ShimWaitDone().

XAieGbl_RegFldAttr XAieGbl_RegShimDmaSts::Stalled

If stalled due to lock.

Referenced by XAieDma_ShimPendingBdCount(), and XAieDma_ShimWaitDone().

XAieGbl_RegFldAttr XAieGbl_RegShimDmaSts::StartQSize

Start queue size.

Referenced by XAieDma_ShimPendingBdCount(), and XAieDma_ShimWaitDone().

XAieGbl_RegFldAttr XAieGbl_RegShimDmaSts::StartQueueOverflow

Start queue overflow.

XAieGbl_RegFldAttr XAieGbl_RegShimDmaSts::Sts

Status.

Referenced by XAieDma_ShimPendingBdCount(), and XAieDma_ShimWaitDone().