| uartns550 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xuartns550.c File Reference

## Functions
int | XUartNs550_CfgInitialize (XUartNs550 *InstancePtr, XUartNs550_Config *Config, UINTPTR EffectiveAddr)
| Initializes a specific XUartNs550 instance such that it is ready to be used. More...
unsigned int | XUartNs550_Send (XUartNs550 *InstancePtr, u8 *BufferPtr, unsigned int NumBytes)
| This functions sends the specified buffer of data using the UART in either polled or interrupt driven modes. More...
unsigned int | XUartNs550_Recv (XUartNs550 *InstancePtr, u8 *BufferPtr, unsigned int NumBytes)
| This function will attempt to receive a specified number of bytes of data from the UART and store it into the specified buffer. More...
unsigned int | XUartNs550_SendBuffer (XUartNs550 *InstancePtr)
| This function sends a buffer that has been previously specified by setting up the instance variables of the instance. More...
unsigned int | XUartNs550_ReceiveBuffer (XUartNs550 *InstancePtr)
| This function receives a buffer that has been previously specified by setting up the instance variables of the instance. More...