| dsirxss Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdsi2rxss_selftest_example.c File Reference

## Overview

This file contains a design example using the XDsi2RxSs driver.

It performs a self test on the MIPI DSI Rx Subsystem that will test its sub-cores self test functions.

Note
  None.

    MODIFICATION HISTORY:

    Ver Who Date    Changes

    1.0 Kunal 12/2/24 Initial Release for MIPI DSI RX subsystem
    1.1 Kunal 18/4/24 Driver name changed to DSI2RXSS.

## Functions
u32 | Dsi2RxSs_SelfTestExample (u32 BaseAddr)
| This function is the main entry point for the self test example using the XDsi2RxSs driver. More...
int | main ()
| This is the main function for XDsiRxSs self test example. More...

## Function Documentation

u32 Dsi2RxSs_SelfTestExample | ( | u32 | BaseAddr | ) |

This function is the main entry point for the self test example using the XDsi2RxSs driver.

This function check whether or not its sub-core drivers self test functions are in working state.

Parameters

  BaseAddress | is the unique Address of the MIPI DSI2 RX . Subsystem core.

Returns
  - XST_FAILURE if any of MIPI DSI RX Subsystem sub-core self test failed.
  - XST_SUCCESS, if all of MIPI DSI RX Subsystem sub-core self test passed.

Note
  None.

References XDsi2RxSs_Config::BaseAddr, XDsi2RxSs_CfgInitialize(), XDsi2RxSs_LookupConfig(), and XDsi2RxSs_SelfTest().

Referenced by main().

int main | ( |  | ) |

This is the main function for XDsiRxSs self test example.

Parameters

  None. |

Returns
  - XST_SUCCESS if the self test example passed.
  - XST_FAILURE if the self test example was unsuccessful.

Note
  None.

References Dsi2RxSs_SelfTestExample().