| v_demosaic Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XV_demosaic_Config Struct Reference

This typedef contains configuration information for the demosaic core Each core instance should have a configuration structure associated. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| The base address of the core instance. More...
u16 | PixPerClk
| Samples Per Clock. More...
u16 | MaxWidth
| Maximum columns supported by core instance. More...
u16 | MaxHeight
| Maximum rows supported by core instance. More...
u16 | MaxDataWidth
| Maximum Data width of each channel. More...
u16 | Algorithm
| Interpolation method. More...

## Detailed Description

This typedef contains configuration information for the demosaic core Each core instance should have a configuration structure associated.

## Field Documentation

u16 XV_demosaic_Config::Algorithm

Interpolation method.

UINTPTR XV_demosaic_Config::BaseAddress

The base address of the core instance.

u16 XV_demosaic_Config::DeviceId

Unique ID of device.

u16 XV_demosaic_Config::MaxDataWidth

Maximum Data width of each channel.

u16 XV_demosaic_Config::MaxHeight

Maximum rows supported by core instance.

u16 XV_demosaic_Config::MaxWidth

Maximum columns supported by core instance.

u16 XV_demosaic_Config::PixPerClk

Samples Per Clock.