| dsi Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Macros | Typedefs | Enumerations | Functions
xdsi.h File Reference

## Data Structures
struct | XDsi_ShortPacket
| This typedef contains the Short Packet information from the Generic Short Packet Register. More...
struct | XDsiTx_CmdModePkt
| MIPI DSI Command Mode configuration structure. More...
struct | XDsi_VideoTiming
| Video timing structure. More...
struct | XDsi_Config
| The configuration structure for DSI Controller This structure passes the hardware building information to the driver. More...
struct | XDsi_ConfigParameters
| The structure to read DSI controller & Configurable Parameters. More...
struct | XDsi
| The XDsi driver instance data. More...

## Macros
#define | NUM_PACKETS 64
| DSI Long packet supports upto 255 word counts - i.e 64 writes into data fifo. More...

## Typedefs
typedef void(* | XDsi_Callback )(void *CallbackRef, u32 Mask)
| Callback type for all interrupts defined. More...

## Enumerations
enum | XDsi_DsiModeType
enum | XDsi_CmdModePktType
enum | XDsi_VideoMode
| Video Timing Mode by default Non-burst mode with Sync Events. More...

## Functions
XDsi_Config * | XDsi_LookupConfig (u32 DeviceId)
| Look up the hardware configuration for a device instance. More...
u32 | XDsi_CfgInitialize (XDsi *InstancePtr, XDsi_Config *CfgPtr, UINTPTR EffectiveAddr)
| Initialize the XDsi instance provided by the caller based on the given Config structure. More...
u32 | XDsi_Activate (XDsi *InstancePtr, XDsi_Selection Flag)
| This function will enable/disable the IP Core to start processing. More...
void | XDsi_Reset (XDsi *InstancePtr)
| This function will do a reset of the IP. More...
u32 | XDsi_DefaultConfigure (XDsi *InstancePtr)
| This function will configure protocol reg with video mode, Blank packet mode, Blank packet Type, End of Transmisstion packet. More...
u32 | XDsi_SelfTest (XDsi *InstancePtr)
| Runs a self-test on the driver/device. More...
void | XDsi_SendShortPacket (XDsi *InstancePtr, XDsi_ShortPacket *ShortPacket)
| This function will send the short packet to DSI controller Generic Short Packet Register. More...
int | XDsi_SendCmdModePkt (XDsi *InstancePtr, XDsiTx_CmdModePkt *CmdPktData)
int | XDsi_SetMode (XDsi *InstancePtr, XDsi_DsiModeType mode)
void | XDsi_GetConfigParams (XDsi *InstancePtr, XDsi_ConfigParameters *ConfigInfo)
| This function will get the information from the GUI settings and other protocol control register values like video mode, Blank packet type, Packet Mode, EOTP value. More...
s32 | XDsi_SetVideoInterfaceTiming (XDsi *InstancePtr, XDsi_VideoMode VideoMode, XVidC_VideoMode Resolution, u16 BurstPacketSize)
| This function Set Timning mode and Resolution as per that it populate with Peripheral Timing Parameters from the video common library. More...
s32 | XDsi_SetCustomVideoInterfaceTiming (XDsi *InstancePtr, XDsi_VideoMode VideoMode, XDsi_VideoTiming *Timing)
| XDsi_SetCustomVideoInterfaceTiming Set Timning mode and Resolution as per user input. More...
s32 | XDsi_SetCallback (XDsi *InstancePtr, u32 HandleType, void *CallbackFunc, void *CallbackRef)
| This routine installs an asynchronous callback function for the given HandlerType: More...