| dfeprach Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfePrach_DecimatorStatusOverflow Struct Reference
Overview

PRACH decimator overflow status. More...

## Data Fields
u32 | DecimatorOverflow
                    [0-1] Source of first occurrence of
overflow as signalled in ISR. More...
u32 | FirstAntennaOverflowing
                          [0-7] Lowest number antenna on which
first overflow occurred. More...
u32 | FirstRCIdOverflowing
                       [0-15] Lowest numbered Physical RACH
channel on which first overrun occurred. More...

## Detailed Description

PRACH decimator overflow status.

## Field Documentation

u32 XDfePrach_DecimatorStatusOverflow::DecimatorOverflow

                    [0-1] Source of first occurrence of

overflow as signalled in ISR.

That is, register only updated when DECIMATOR_OVERFLOW flag is 0.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_DecimatorStatusOverflow::FirstAntennaOverflowing

                          [0-7] Lowest number antenna on which

first overflow occurred.

Referenced by XDfePrach_GetStatus().

u32 XDfePrach_DecimatorStatusOverflow::FirstRCIdOverflowing

                       [0-15] Lowest numbered Physical RACH

channel on which first overrun occurred.

Referenced by XDfePrach_GetStatus().