| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_CCSequence Struct Reference
Overview

Defines a CCID sequence. More...

## Data Fields
u32 | Length
| [1-16] Sequence length. More...
s32 | CCID [XDFEMIX_SEQ_LENGTH_MAX]
       [0-15].Array of CCID's
arranged in the order the CCIDs are required to be processed in the DUC/DDC Mixer. More...
s32 | NotUsedCCID
| Lowest CCID number not allocated. More...

## Detailed Description

Defines a CCID sequence.

## Field Documentation

s32 XDfeMix_CCSequence::CCID[XDFEMIX_SEQ_LENGTH_MAX]

       [0-15].Array of CCID's

arranged in the order the CCIDs are required to be processed in the DUC/DDC Mixer.

Referenced by XDfeMix_GetCarrierCfgAndNCO(), and XDfeMix_GetEmptyCCCfg().

u32 XDfeMix_CCSequence::Length

[1-16] Sequence length.

Referenced by XDfeMix_AddCCExample(), XDfeMix_GetCarrierCfgAndNCO(), XDfeMix_GetEmptyCCCfg(), XDfeMix_Initialize(), and XDfeMix_MultiAddCCExample().

s32 XDfeMix_CCSequence::NotUsedCCID

Lowest CCID number not allocated.

Referenced by XDfeMix_AddCC(), XDfeMix_GetCurrentCCCfg(), XDfeMix_GetCurrentCCCfgSwitchable(), XDfeMix_MoveCC(), XDfeMix_RemoveCC(), XDfeMix_SetNextCCCfgAndTrigger(), XDfeMix_SetNextCCCfgAndTriggerSwitchable(), and XDfeMix_UpdateCC().