| dfeccf Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeCcf_Status Struct Reference
Overview

Event status and interrupt mask. More...

## Data Fields
u32 | Overflow
| [0,1] Mask overflow events More...
u32 | CCUpdate
| [0,1] Mask CC update events More...
u32 | CCSequenceError
| [0,1] Mask CC sequence mismatch events More...

## Detailed Description

Event status and interrupt mask.

Note
  The structure for XDfeCcf_InterruptMask is the same as that of XDfeCcf_Status

## Field Documentation

u32 XDfeCcf_Status::CCSequenceError

[0,1] Mask CC sequence mismatch events

Referenced by XDfeCcf_ClearEventStatus(), XDfeCcf_GetEventStatus(), XDfeCcf_GetInterruptMask(), XDfeCcf_multiAddCC_1xNR100_3xNR20_Example(), XDfeCcf_PassThroughExample(), and XDfeCcf_SetInterruptMask().

u32 XDfeCcf_Status::CCUpdate

[0,1] Mask CC update events

Referenced by XDfeCcf_ClearEventStatus(), XDfeCcf_GetEventStatus(), XDfeCcf_GetInterruptMask(), XDfeCcf_multiAddCC_1xNR100_3xNR20_Example(), XDfeCcf_PassThroughExample(), and XDfeCcf_SetInterruptMask().

u32 XDfeCcf_Status::Overflow

[0,1] Mask overflow events

Referenced by XDfeCcf_ClearEventStatus(), XDfeCcf_GetEventStatus(), XDfeCcf_GetInterruptMask(), XDfeCcf_multiAddCC_1xNR100_3xNR20_Example(), XDfeCcf_PassThroughExample(), and XDfeCcf_SetInterruptMask().