| sdi_common Vitis Drivers API Documentation

- Overview
- APIs
- File List

Enumerations | Variables
Overview

## Enumerations
enum | XSdiVid_Standard
| Payload and digital interface standards. More...
enum | XSdiVid_TransMode
| SDI Modes. More...
enum | XSdiVid_BitRate
| Channel Assignment. More...
enum | XSdiVid_ChannelAssignment
| Channel Assignment. More...
enum | XSdiVid_Eotf
| End of Transfer Characteristics. More...

## Variables
const XVidC_VideoTimingMode | XVidC_SdiVidTimingModes [XVIDC_SDICUSTOM_NUM_SUPPORTED]
| SDI Specific 3GB timing modes. More...
const XVidC_VideoTimingMode | XVidC_SdiVidTimingModes [XVIDC_SDICUSTOM_NUM_SUPPORTED]
| SDI Specific 3GB timing modes. More...

## Enumeration Type Documentation

enum XSdiVid_BitRate

Channel Assignment.

enum XSdiVid_ChannelAssignment

Channel Assignment.

enum XSdiVid_Eotf

End of Transfer Characteristics.

enum XSdiVid_Standard

Payload and digital interface standards.

enum XSdiVid_TransMode

SDI Modes.

## Variable Documentation

const XVidC_VideoTimingMode XVidC_SdiVidTimingModes[XVIDC_SDICUSTOM_NUM_SUPPORTED]

Initial value:
=
{
{ XVIDC_VM_1920x1080_96_I, "1920x1080@96Hz (I)", XVIDC_FR_96HZ,
{1920, 371, 88, 371, 2750, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
{ XVIDC_VM_1920x1080_100_I, "1920x1080@100Hz (I)", XVIDC_FR_100HZ,
{1920, 528, 44, 148, 2640, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
{ XVIDC_VM_1920x1080_120_I, "1920x1080@120Hz (I)", XVIDC_FR_120HZ,
{1920, 88, 44, 148, 2200, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
{ XVIDC_VM_2048x1080_96_I, "2048x1080@96Hz (I)", XVIDC_FR_96HZ,
{2048, 329, 44, 329, 2750, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
{ XVIDC_VM_2048x1080_100_I, "2048x1080@100Hz (I)", XVIDC_FR_100HZ,
{2048, 274, 44, 274, 2640, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
{ XVIDC_VM_2048x1080_120_I, "2048x1080@120Hz (I)", XVIDC_FR_120HZ,
{2048, 66, 20, 66, 2200, 1,
1080, 5, 10, 30, 1125, 5, 10, 30, 1125, 1} },
}

SDI Specific 3GB timing modes.

const XVidC_VideoTimingMode XVidC_SdiVidTimingModes[XVIDC_SDICUSTOM_NUM_SUPPORTED]

SDI Specific 3GB timing modes.