| v_hdmitxss1 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Data Structures | Macros | Typedefs | Enumerations
xhdmi_example.h File Reference

## Overview

This file contains set of definition for the main application.

    MODIFICATION HISTORY:

    Ver   Who    Date     Changes
                 dd/mm/yy

    1.00  YB     11/05/19 Initial release.

## Data Structures
struct | XHdmi_Exdes
| This typedef defines the handler for the pass-thorugh example design that handles the state of the pass-through design. More...

## Macros
#define | _XHDMI_EXAMPLE_H_
| prevent circular inclusions by using protection macros More...
#define | I2C_MUX_ADDR 0x74
| I2C Mux Address. More...
#define | I2C_CLK_ADDR 0x7C
| I2C Clk Address IDT_8T49N241. More...
#define | I2C_CLK_ADDR1 0x6C
| I2C Clk Address IDT_8T49N241. More...
#define | FVA_FACTOR 1
| Note : In Auto Stretch Mode, Enable/Disable VRR is not supported. More...
#define | RC21008A_ADDR 0x09
| I2C RC21008A Address. More...

## Typedefs
typedef void(* | Exdes_Debug_Printf )(const char *fmt,...)
| Define a function pointer for user enabled printing. More...

## Enumerations
enum | TxInputSourceType
| This enumeration defines the 'type' of sources that can provide a video stream for the transmitter to output in the example design. More...
enum | DynamicHDRType
| This enmueration defines the Dynamic HDR TYPE. More...

## Macro Definition Documentation

#define _XHDMI_EXAMPLE_H_

prevent circular inclusions by using protection macros

#define FVA_FACTOR 1

Note : In Auto Stretch Mode, Enable/Disable VRR is not supported.

VRR/FSYNC is always on in VTEM/AMD VSIF Packet

#define I2C_CLK_ADDR 0x7C

I2C Clk Address IDT_8T49N241.

Referenced by I2cClk().

#define I2C_CLK_ADDR1 0x6C

I2C Clk Address IDT_8T49N241.

Referenced by I2cClk().

#define I2C_MUX_ADDR 0x74

I2C Mux Address.

#define RC21008A_ADDR 0x09

I2C RC21008A Address.

Referenced by Exdes_SetupClkSrc().

## Typedef Documentation

typedef void(* Exdes_Debug_Printf)(const char *fmt,...)

Define a function pointer for user enabled printing.

## Enumeration Type Documentation

enum DynamicHDRType

This enmueration defines the Dynamic HDR TYPE.

enum TxInputSourceType

This enumeration defines the 'type' of sources that can provide a video stream for the transmitter to output in the example design.