| dfeequ Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeEqu_Status Struct Reference
Overview

Equalizer Status. More...

## Data Fields
u32 | IStatus [XDFEEQU_CHANNEL_NUM]
          bit0 is overflow of I datapath
and bit 1 is overflow of Q datapath in real mode only. More...
u32 | QStatus [XDFEEQU_CHANNEL_NUM]
          Overflow of Q datapath in
complex mode. More...

## Detailed Description

Equalizer Status.

## Field Documentation

u32 XDfeEqu_Status::IStatus[XDFEEQU_CHANNEL_NUM]

          bit0 is overflow of I datapath

and bit 1 is overflow of Q datapath in real mode only.

Referenced by XDfeEqu_ClearEventStatus(), and XDfeEqu_GetEventStatus().

u32 XDfeEqu_Status::QStatus[XDFEEQU_CHANNEL_NUM]

          Overflow of Q datapath in

complex mode.

Referenced by XDfeEqu_ClearEventStatus(), and XDfeEqu_GetEventStatus().