| rfdc Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xrfdc_intr.c File Reference

## Functions
u32 | XRFdc_IntrEnable (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 Block_Id, u32 IntrMask)
| This function sets the interrupt mask. More...
u32 | XRFdc_IntrDisable (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 Block_Id, u32 IntrMask)
| This function clears the interrupt mask. More...
u32 | XRFdc_GetEnabledInterrupts (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 Block_Id, u32 *IntrMask)
| This function gets a mask of enabled interrupts. More...
u32 | XRFdc_GetIntrStatus (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 Block_Id, u32 *IntrStsPtr)
| This function returns the interrupt status read from Interrupt Status Register(ISR). More...
u32 | XRFdc_IntrClr (XRFdc *InstancePtr, u32 Type, u32 Tile_Id, u32 Block_Id, u32 IntrMask)
| This function clear the interrupts. More...
u32 | XRFdc_IntrHandler (u32 Vector, void *XRFdcPtr)
| This function is the interrupt handler for the driver. More...
void | XRFdc_SetStatusHandler (XRFdc *InstancePtr, void *CallBackRef, XRFdc_StatusHandler FunctionPtr)
| This function sets the status callback function, the status handler, which the driver calls when it encounters conditions that should be reported to the higher layer software. More...