| mipi_tx_phy Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xmipi_tx_phy_example_selftest.c File Reference

## Overview

    MODIFICATION HISTORY:

    Ver   Who       Date     Changes

    1.1    pg    16/02/24 Initial release - Application initializes mipi_tx_phy
                           and ensures register reads and writes are good.

## Functions
u32 | Mipi_Tx_PhySelfTestExample (UINTPTR BaseAddress)
| This function checks if the HS_TIMEOUT from the generated file matches the value present in the corresponding configuration register. More...
int | main ()
| The entry point for this example. More...

## Function Documentation

int main | ( |  | ) |

The entry point for this example.

It invokes the example function, and reports the execution status.

Parameters

  None. |

Returns
  - XST_SUCCESS if example finishes successfully
  - XST_FAILURE if example fails.

Note
  None.

References Mipi_Tx_PhySelfTestExample().

u32 Mipi_Tx_PhySelfTestExample | ( | UINTPTR | BaseAddress | ) |

This function checks if the HS_TIMEOUT from the generated file matches the value present in the corresponding configuration register.

Parameters

  BaseAddress | is the Mipi_Tx_Phy BaseAddress.

Returns
  - XST_SUCCESS if values match

- XST_FAILURE if values differ.

Note
  None.

References XMipi_Tx_Phy_Config::BaseAddr, XMipi_Tx_Phy_CfgInitialize(), XMipi_Tx_Phy_GetRegIntfcPresent(), XMipi_Tx_Phy_LookupConfig(), and XMipi_Tx_Phy_SelfTest().

Referenced by main().