| axidma Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

File List
Here is a list of all documented files with brief descriptions:

xaxidma.c |
xaxidma.h |
xaxidma_bd.c |
xaxidma_bd.h |
xaxidma_bdring.c |
xaxidma_bdring.h |
xaxidma_example_poll_multi_pkts.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer multiple packets in polling mode when the AXI DMA core is configured in Scatter Gather Mode
xaxidma_example_selftest.c | This file demonstrates the example to do selftest on the device
xaxidma_example_sg_intr.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer packets in interrupt mode when the AXIDMA core is configured in Scatter Gather Mode
xaxidma_example_sg_poll.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer packets in polling mode when the AXIDMA core is configured in Scatter Gather Mode
xaxidma_example_sgcyclic_intr.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer packets in interrupt mode when the AXIDMA core is configured in Scatter Gather Mode
xaxidma_example_simple_intr.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer packets.in interrupt mode when the AXIDMA core is configured in simple mode
xaxidma_example_simple_poll.c | This file demonstrates how to use the xaxidma driver on the Xilinx AXI DMA core (AXIDMA) to transfer packets in polling mode when the AXI DMA core is configured in simple mode
xaxidma_g.c |
xaxidma_hw.h |
xaxidma_porting_guide.h |
xaxidma_selftest.c |
xaxidma_sinit.c |