| tmrctr Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XTmrCtr_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| Register base address. More...
u32 | SysClockFreqHz
| The AXI bus clock frequency. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

UINTPTR XTmrCtr_Config::BaseAddress

Register base address.

Referenced by XTmrCtr_CfgInitialize(), and XTmrCtr_Initialize().

u16 XTmrCtr_Config::DeviceId

Unique ID of device.

u32 XTmrCtr_Config::SysClockFreqHz

The AXI bus clock frequency.

Referenced by XTmrCtr_PwmConfigure().