| uartlite Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XUartLite_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | RegBaseAddr
| Register base address. More...
u32 | BaudRate
| Fixed baud rate. More...
u8 | UseParity
| Parity generator enabled when TRUE. More...
u8 | ParityOdd
| Parity generated is odd when TRUE, even when FALSE. More...
u8 | DataBits
| Fixed data bits. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XUartLite_Config::BaudRate

Fixed baud rate.

u8 XUartLite_Config::DataBits

Fixed data bits.

u16 XUartLite_Config::DeviceId

Unique ID of device.

u8 XUartLite_Config::ParityOdd

Parity generated is odd when TRUE, even when FALSE.

UINTPTR XUartLite_Config::RegBaseAddr

Register base address.

Referenced by XUartLite_Initialize().

u8 XUartLite_Config::UseParity

Parity generator enabled when TRUE.