| devcfg Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdevcfg_hw.c File Reference

## Functions
void | XDcfg_ResetHw (u32 BaseAddr)
| This function perform the reset sequence to the given devcfg interface by configuring the appropriate control bits in the devcfg specifc registers the devcfg reset squence involves the following steps Disable all the interuupts Clear the status Update relevant config registers with reset values Disbale the looopback mode and pcap rate enable. More...