| dp21 Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XDp_TxLttprConfig Struct Reference
Overview

This typedef contains configuration information about the main link settings. More...

## Data Fields
u8 | RevId
| The LTTPR Capability and ID Field. More...
u8 | MaxLinkRate_8B
| The maximum link rate for 8B LTTPR encoding. More...
u8 | RepeaterCnt
| Indicates the number of LTTPR's that are present. More...
u8 | RepeaterMode
| LTTPR repeater mode. More...
u8 | MaxLaneCount
| The maximum lane count of LTTPR. More...
u8 | ExtendTimeOut
| The Repeater Extended timeout. More...
u8 | ChannelCoding
| The Main Link channel coding of LTTPR. More...
u8 | MaxLinkRate_128B
| LTTPR Linkrate for 128B channel encoding. More...
u8 | EqDone
| Equiliation Done per LTTPR. More...
u8 | AlpmCapabilities
| AUX-Less ALPM Capabilities. More...
u8 | TotalRptCnt
| Total LTTPR count. More...
u8 | reserved_bytes [6]
| Reserved. More...

## Detailed Description

This typedef contains configuration information about the main link settings.

## Field Documentation

u8 XDp_TxLttprConfig::AlpmCapabilities

AUX-Less ALPM Capabilities.

u8 XDp_TxLttprConfig::ChannelCoding

The Main Link channel coding of LTTPR.

u8 XDp_TxLttprConfig::EqDone

Equiliation Done per LTTPR.

u8 XDp_TxLttprConfig::ExtendTimeOut

The Repeater Extended timeout.

u8 XDp_TxLttprConfig::MaxLaneCount

The maximum lane count of LTTPR.

u8 XDp_TxLttprConfig::MaxLinkRate_128B

LTTPR Linkrate for 128B channel encoding.

u8 XDp_TxLttprConfig::MaxLinkRate_8B

The maximum link rate for 8B LTTPR encoding.

u8 XDp_TxLttprConfig::RepeaterCnt

Indicates the number of LTTPR's that are present.

u8 XDp_TxLttprConfig::RepeaterMode

LTTPR repeater mode.

u8 XDp_TxLttprConfig::reserved_bytes[6]

Reserved.

u8 XDp_TxLttprConfig::RevId

The LTTPR Capability and ID Field.

u8 XDp_TxLttprConfig::TotalRptCnt

Total LTTPR count.