| dmaps Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdmaps_hw.c File Reference

## Functions
void | XDmaPs_ResetHw (u32 BaseAddress)
| This function perform the reset sequence to the given dmaps interface by configuring the appropriate control bits in the dmaps specifc registers the dmaps reset squence involves the following steps Disable all the interuupts Clear the pending interrupts Kill all the active channel threads Kill the manager thread. More...