| dfemix Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XDfeMix_DUCDDCCfg Struct Reference
Overview

Defines settings for single CC's DUC/DDC. More...

## Data Fields
u32 | NCOIdx
| [0-7] DUC/DDC NCO assignment More...
u32 | CCGain
| [0-3] Adjust gain of CCID after mixing (applies to all antennas for that CCID). More...

## Detailed Description

Defines settings for single CC's DUC/DDC.

## Field Documentation

u32 XDfeMix_DUCDDCCfg::CCGain

[0-3] Adjust gain of CCID after mixing (applies to all antennas for that CCID).

Only applicable to downlink.

- 0 = MINUS18DB: Apply -18dB gain.
- 1 = MINUS12DB: Apply -12dB gain.
- 2 = MINUS6DB: Apply -6dB gain.
- 3 = ZERODB: Apply -0dB gain.

Referenced by XDfeMix_AddCC(), XDfeMix_AddCCExample(), XDfeMix_GetCarrierCfgAndNCO(), XDfeMix_MultiAddCCExample(), and XDfeMix_UpdateCC().

u32 XDfeMix_DUCDDCCfg::NCOIdx

[0-7] DUC/DDC NCO assignment

Referenced by XDfeMix_AddCC(), XDfeMix_AddCCExample(), XDfeMix_AddCCtoCCCfg(), XDfeMix_GetCarrierCfgAndNCO(), XDfeMix_MultiAddCCExample(), XDfeMix_UpdateCC(), and XDfeMix_UpdateCCinCCCfg().