| tft Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XTft_Config Struct Reference
Overview

This structure holds the Device base address, video memory base address and Unique identifier of the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| Base address of device. More...
UINTPTR | VideoMemBaseAddr
| Video Memory Base address. More...
u32 | AddrWidth
| Address Width. More...

## Detailed Description

This structure holds the Device base address, video memory base address and Unique identifier of the device.

## Field Documentation

u32 XTft_Config::AddrWidth

Address Width.

Referenced by XTft_SetFrameBaseAddr().

UINTPTR XTft_Config::BaseAddress

Base address of device.

Referenced by TftExample(), XTft_CfgInitialize(), XTft_ReadReg(), and XTft_WriteReg().

u16 XTft_Config::DeviceId

Unique ID of device.

Referenced by XTft_CfgInitialize().

UINTPTR XTft_Config::VideoMemBaseAddr

Video Memory Base address.

Referenced by XTft_CfgInitialize(), XTft_GetPixel(), XTft_SetFrameBaseAddr(), and XTft_SetPixel().