| csi2tx Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xcsi2tx.c File Reference

## Functions
u32 | XCsi2Tx_CfgInitialize (XCsi2Tx *InstancePtr, XCsi2Tx_Config *CfgPtr, UINTPTR EffectiveAddr)
| Initialize the XCsi2Tx instance provided by the caller based on the given Config structure. More...
u32 | XCsi2Tx_Reset (XCsi2Tx *InstancePtr)
| This function will do a reset of the IP. More...
u32 | XCsi2Tx_Activate (XCsi2Tx *InstancePtr, u8 Flag)
| Thsi function will enable/disable the IP Core to start processing. More...
u32 | XCsi2Tx_Configure (XCsi2Tx *InstancePtr)
| This function will configure the core with proper number of Active Lanes. More...
void | XCsi2Tx_GetShortPacket (XCsi2Tx *InstancePtr, XCsi2Tx_SPktData *ShortPacketStruct)
| This function will get the short packet received in the FIFO from the Generic Short Packet Register and fill up the structure passed from caller. More...
u8 | XCsi2Tx_IsActiveLaneCountValid (XCsi2Tx *InstancePtr, u8 ActiveLanesCount)
| This function checks the validity of the active lanes parameter. More...
u32 | XCsi2Tx_SetLineCountForVC (XCsi2Tx *InstancePtr, u8 VC, u16 LineCount)
| This function sets the Line Count for virtual Channel if Frame End Generation feature is enabled. More...
u32 | XCsi2Tx_GetLineCountForVC (XCsi2Tx *InstancePtr, u8 VC, u16 *LineCount)
| This function gets the Line Count for virtual Channel if Frame End Generation feature is enabled. More...