| v_hdmi_common Vitis Drivers API Documentation

- Overview
- Data Structures

- Data Structures
- Data Fields

Data Fields
XHdmiC_VSIF Struct Reference

Structure for holding the VSIF. More...

## Data Fields
u8 | Version
| Version. More...
XHdmiC_IEEE_Id_Type | IEEE_ID
| IEEE Registration Identifier. More...
u8 | Is_3D_Valid
| Indicates Valid 3D data present. More...
u8 | ALLM_Mode
| The Source shall use this field to enable and disable the Sinkâ?Ts ALLM. More...
u8 | CCBPC
| Color Content Bits per Component. More...
XHdmiC_VSIF_Video_Format | Format
| HDMI Video Format. More...
u8 | HDMI_VIC
| XHDMIC_VSIF_VF_EXTRES: HDMI Video Format Identification Code. More...
XHdmiC_3D_Info | Info_3D
| XHDMIC_VSIF_VF_3D: 3D Information. More...

## Detailed Description

Structure for holding the VSIF.

Format indicates the used union member.

## Field Documentation

u8 XHdmiC_VSIF::ALLM_Mode

The Source shall use this field to enable and disable the Sinkâ?Ts ALLM.

u8 XHdmiC_VSIF::CCBPC

Color Content Bits per Component.

XHdmiC_VSIF_Video_Format XHdmiC_VSIF::Format

HDMI Video Format.

u8 XHdmiC_VSIF::HDMI_VIC

XHDMIC_VSIF_VF_EXTRES: HDMI Video Format Identification Code.

XHdmiC_IEEE_Id_Type XHdmiC_VSIF::IEEE_ID

IEEE Registration Identifier.

XHdmiC_3D_Info XHdmiC_VSIF::Info_3D

XHDMIC_VSIF_VF_3D: 3D Information.

u8 XHdmiC_VSIF::Is_3D_Valid

Indicates Valid 3D data present.

u8 XHdmiC_VSIF::Version

Version.