| scutimer Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XScuTimer_Config Struct Reference
Overview

This typedef contains configuration information for the device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
u32 | BaseAddr
| Base address of the device. More...

## Detailed Description

This typedef contains configuration information for the device.

## Field Documentation

u32 XScuTimer_Config::BaseAddr

Base address of the device.

Referenced by ScuTimerIntrExample(), ScuTimerPolledExample(), XScuTimer_CfgInitialize(), XScuTimer_GetPrescaler(), XScuTimer_SelfTest(), XScuTimer_SetPrescaler(), XScuTimer_Start(), and XScuTimer_Stop().

u16 XScuTimer_Config::DeviceId

Unique ID of device.

Referenced by XScuTimer_CfgInitialize().