| board_common Vitis Drivers API Documentation

- Overview
- APIs
- File List
- Examples

Examples

You can refer to the below stated example applications for more details on how to use rfclk driver.

# xrfclk_example_app.c

Contains an example on how to use the XRfclk driver directly on clk104 daughter board on zcu216. This example does the following:

- configure LMK and LMX,
- read LMK and LMX configurations,
- read/write registers for LMK and LMX,
- reset LMK and LMX

For details, see xrfclk_example_app.c.