| usbpsu Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xusb_composite_example.c File Reference

## Overview

This file implements mass storage, hid, audio and dfu all in one composite device.

    MODIFICATION HISTORY:

    Ver   Who  Date     Changes

    1.0   rb   05/03/18 First release
    1.14  pm   21/06/23 Added support for system device-tree flow.

## Functions
int | main (void)
| This function is the main function of the AUDI-DFU composite example. More...

## Function Documentation

int main | ( | void |  | ) |

This function is the main function of the AUDI-DFU composite example.

Parameters

  None. |

Returns
  - XST_SUCCESS if successful,
  - XST_FAILURE if unsuccessful.

Note
  None.