| emaclite Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xemaclite_ping_reply_example.c File Reference

## Overview

This file contains an EmacLite ping reply example in polled mode.

This example will generate a ping reply when it receives a ping request packet from the external world.

Note

The local IP address is set to 172.16.63.121. User needs to update LocalIpAddr variable with a free IP address based on the network on which this example is to be run.

The local MAC address is set to 0x000A35030201. User can update LocalMacAddr variable with a valid MAC address. The first three bytes contains the manufacture ID. 0x000A35 is XILINX manufacture ID.

This program will respond continuously to a number of ping requests as defined by MAX_PING_REPLIES in this file.

    MODIFICATION HISTORY:

    Ver   Who  Date     Changes

    1.00a ktn  20/08/08 First release
    3.00a ktn  10/22/09 Updated example to use the macros that have been changed
                  in the driver to remove _m from the name of the macro.
    3.01a ktn  08/06/10 Updated the example to support little endian MicroBlaze.
    4.3   ms   01/23/17 Added xil_printf statement in main function to
                        ensure that "Successfully ran" and "Failed" strings
                        are available in all examples. This is a fix for
                        CR-965028.

## Functions
int | main ()
| This function is the main function of the Ping reply example in polled mode. More...

## Function Documentation

int main | ( | void |  | ) |

This function is the main function of the Ping reply example in polled mode.

Parameters

  None. |

Returns
  XST_FAILURE to indicate failure, otherwise XST_SUCCESS is returned.

Note
  None.