| dsi Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

Functions
xdsi_example_selftest.c File Reference

## Overview

Note
  None.

    MODIFICATION HISTORY:

    Ver  Who Date     Changes

    1.1  ms  01/23/17 Modified xil_printf statement in main function to
                      ensure that "Successfully ran" and "Failed" strings
                      are available in all examples. This is a fix for
                      CR-965028.
         ms  04/05/17 Modified Comment lines in functions to
                      recognize it as documentation block for doxygen
                      generation of examples.

## Functions
u32 | DsiSelfTestExample (u32 DeviceId)
| This function will perform DSI self test prints GUI parameters. More...
int | main ()
| The entry point for this example. More...

## Function Documentation

u32 DsiSelfTestExample | ( | u32 | DeviceId | ) |

This function will perform DSI self test prints GUI parameters.

Parameters

  DeviceId | is the DSI Controller Device id.

Returns
  - XST_SUCCESS if Lane Count match
  - XST_FAILURE if Lane Count don't match.

Note
  None.

References XDsi_Config::BaseAddr, XDsi_CfgInitialize(), XDsi_LookupConfig(), and XDsi_SelfTest().

Referenced by main().

int main | ( |  | ) |

The entry point for this example.

It invokes the example function, and reports the execution status.

Parameters

  None. |

Returns
  - XST_SUCCESS if example finishes successfully
  - XST_FAILURE if example fails.

Note
  None.

References DsiSelfTestExample().