| can Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List
- Examples

- Data Structures
- Data Fields

Data Fields
XCan_Config Struct Reference
Overview

This typedef contains configuration information for a device. More...

## Data Fields
u16 | DeviceId
| Unique ID of device. More...
UINTPTR | BaseAddress
| Register base address. More...
u8 | NumOfAcceptFilters
| Number of Acceptance Filters. More...
u8 | EnableECC
| ECC is enabled or disabled. More...

## Detailed Description

This typedef contains configuration information for a device.

## Field Documentation

UINTPTR XCan_Config::BaseAddress

Register base address.

Referenced by XCan_Initialize().

u16 XCan_Config::DeviceId

Unique ID of device.

u8 XCan_Config::EnableECC

ECC is enabled or disabled.

u8 XCan_Config::NumOfAcceptFilters

Number of Acceptance Filters.