| v_hcresampler Vitis Drivers API Documentation

- Overview
- Data Structures
- APIs
- File List

- Data Structures
- Data Fields

Data Fields
XV_hcresampler Struct Reference

Driver instance data. More...

## Data Fields
XV_hcresampler_Config | Config
| Hardware Configuration. More...
u32 | IsReady
| Device is initialized and ready. More...

## Detailed Description

Driver instance data.

An instance must be allocated for each core in use.

## Field Documentation

XV_hcresampler_Config XV_hcresampler::Config

Hardware Configuration.

Referenced by XV_HCrsmplDbgReportStatus(), XV_HCrsmplLoadDefaultCoeff(), XV_HCrsmplrLoadExtCoeff(), and XV_HCrsmplSetFormat().

u32 XV_hcresampler::IsReady

Device is initialized and ready.